USER GUIDE BOARD UPDATE FIRMWARE

1. When you plugin your power, you hear a “BIP”-> System start OK.

2. After you plug BOARD UPDATE into iTracking board. You must press RESET button in iTracking board and then you press START button in BOARD UPDATE.

When detected device you can hear two short “BIP” and process update is begin, LED Yellow toggle.

Wait for some seconds you can hear:

1. 1 “BIP” and LED Green working mean updated success.

2. 2 “BIP”(1 short 1 long) LED RED working mean update fail and program auto start again. Now you just only press RESET button in iTracking board to begin process update again.